{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"merged":[[1,0,6,0],[4,1,6,1],[7,0,14,0],[19,0,25,0],[19,4,25,4],[28,0,36,0]]}
["项目","购买器材","规   格","数量","备    注"]
[" 电工仪表安全使用（K11）","钳形电流表","0.1—100A数字式",4]
[null,"接地电阻测试仪","ZC29B-1",4]
[null,"直流单臂电桥","QJ23A",4]
[null,"兆欧表","2500伏ZC11D-10",4]
[null,null,"100伏ZC25-4",4]
[null,null,"500伏zc25-3",4]
["安全工具","验电笔","10千伏",4]
[null,"高压放电棒","10-35",3]
[null,"防护眼镜",null,5]
[null,"绝缘棒","4节6米",3]
[null,null,"4节5米",3]
[null,"携带三相短路接地线","1.5*3+7带地丁夹子",1]
[null,"脚扣",null,"2付"]
[null,"绝缘垫 ","1*5米整卷",2]
["电工安全标示的辨识（K13）","各类标示牌",null,"两副"]
["安全操作技术（K2）","模拟图版更新，开关柜修理及双重命名制作",null,"1套"]
[" 10kV高压开关柜的停（送）电操作（21）","开关柜修理","出线柜负荷开关调换"]
[" 10kV高压成套配电装置的巡视检查（K22）","安全帽、戴绝缘手套和绝缘靴",null,"各5套"]
[" 10kV柱上变压器的停（送）电操作（K23）","高压变压器","S1110kV/0.430kVA",1,"需要安装"]
[null,"跌落式熔断器","RW12-12/200A",4]
[null,"高压熔丝","200A","20根"]
[null,"配电箱","2路线电容补偿",1]
[null,"避雷器","10千伏氧化锌",3]
[null,"接地妆及引线",null,1]
[null,"工程安装调试","立杆，安装金具等"]
[" 变压器绝缘测量（K26）","变压器","S11-M-160KVA 10/0.4","1台"]
[null,"变压器工程安装",null,"1套"]
[" 导线在绝缘子上绑扎（K29）","保护接地线",null,1]
[null,"高空防坠器","15米",2]
[null,"双钩紧线器",null,2]
[null,"液压钳","YQK-240/300",1]
[null,"手板葫芦","1吨0.75T手动倒链3米1.5m2",1]
[null,"卡线器",null,2]
[null,"地线卡线器",null,2]
[null,"线路金具,",null,"1台"]
[null,"导线，电缆",null,"1套"]
[null,"海绵垫","高密加厚","1套"]
[" 结合实际工作任务，排除作业现场存在的安全风险、职业病危害（K32）","安全带及安全护栏等","1.2米*3米","各5套"]
["触电急救","模拟人","CPR480","2个"]
[null,"灭火器",null,"10个"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}